Please visit www.objectivesounds.co.uk for more information.

Transferred on the 30th of December 2015

2.8 mil TE at 5g

Speed correct	F4	249Hz

Recorded 4th of April 1939.

Problem Parts

Brass. Careful adjustment necessary. Constant noise threshold necessary.

DC	48	X2
DCRK	45	X2
DNLF	-40dB	150Hz
DN	Constant floor	-50dB floor	-10dB reduction

9K	LP
45	HP
